{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["铝合金门窗维修","后勤为序材料","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"铝合金门窗维修","index":0,"n_rows":12,"n_cols":3,"rows_kept":12,"merged":[[0,0,0,1]],"flags":["formulas_cached_only"]}
["型材规格目录"]
["序号","规格","报价（元）"]
[1,"铝合金隔断，方管80*44型材厚度1.2壁厚，铝合金扣板壁厚1.0厚，玻璃5毫米壁厚钢化玻璃"]
[2,"不锈钢架子，方管40*40型材304材厚度壁厚1.0"]
[3,"不锈钢架子，方管40*40型材202材厚度壁厚1.0"]
[4,"钢化玻璃门，门玻璃厚度壁厚12毫米钢化玻璃皇冠地弹簧\n220B型号地弹簧，304拉手上下夹头皇冠牌"]
[5,"不锈钢304伸缩门，方管25*13型材壁厚1.0"]
[6,"金钢网纱窗三推铝型材25*15型材壁厚1.0纱网304材质壁厚0.6网"]
[7,"防滑板做斜坡材质壁厚8毫米"]
[8,"不锈钢栏杆304材质，圆管63，壁厚1.2厚；圆管51壁厚1.0厚；圆管32壁厚0.8厚"]
[9,"不锈钢水池盆304材质，方管38*25型材厚度1.2壁厚，材质厚度1.0壁厚"]
[10,"不锈钢感应门，玻璃门12毫米不锈钢板材包边\n202材质壁厚1.0，轨道壁厚3毫米，进口吊轮，进口皇冠电机"]

{"sheet":"后勤为序材料","index":1,"n_rows":48,"n_cols":4,"rows_kept":48,"flags":["formulas_cached_only"]}
["物资名称","品牌","规格型号","报价（元）"]
["PVC管",null,20]
["PVC管",null,25]
["电缆",null,"4*35+1"]
["电箱",null,"50*60"]
["电箱",null,"60*80"]
["断路器",null,"100a"]
["断路器",null,"160内六角"]
["断路器",null,"200a内六角"]
["断路器",null,"内六角"]
["多股线",null,1.5]
["多股线",null,2.5]
["多股线",null,4]
["多股线",null,"10平方"]
["护套线",null,"2*1"]
["护套线",null,"2*1.5"]
["护套线",null,"3*1.5"]
["护套线",null,"3*2.5"]
["护套线",null,"3*4圆护套"]
["护套线",null,"圆"]
["护套线",null,"圆3*25"]
["集成吊顶方灯",null,"30*60"]
["接触器",null,"加辅助触头"]
["接触器",null,"(空白)"]
["接地线",null,1.5]
["接地线",null,2.5]
["接地线",null,"1.5平方软线"]
["接地线",null,"2.5平方软线"]
["明箱",null,"50*60"]
["平板灯",null,"30*60"]
["平板灯",null,"60*60"]
["热容球阀",null,25]
["软护套",null,"2*1.5"]
["软线",null,2.5]
["软线",null,4]
["软线",null,6]
["软线",null,"10平方"]
["软线",null,"2.5平方"]
["软线",null,"4平方"]
["软线",null,"6平方"]
["漏电保护器",null,"(空白)"]
["数显万用表",null,"(空白)"]
["双排电箱",null,"(空白)"]
["水槽",null,"不锈钢双水槽"]
["网线",null,"6类"]
["线管",null,16]
["鸭嘴跳线+钳子",null,"(空白)"]
["增压泵",null,"(空白)"]

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}